**DAILY ASSESSMENT FORMAT**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date:** | 5/29/20 | **Name:** | **Sathya br** |
| **Course:** | **LOGIC DESIGN** | **USN:** | **4al16ec065** |
| **Topic:** | **Boolean equations for digital circuits.**  **Combinational circuits: Conversion of MUX and Decoders to logic gates.**  **design of 7 segment decoder with common anode display** | **Semester & Section:** | **6th seminar**  **B section** |
| **Github Repository:** | **sathyabr** |  |  |

|  |
| --- |
| **FORENOON SESSION DETAILS** |
| **Image of session** |
| **Report – Report can be typed or hand written for up to two pages.**  **Boolean equations for digital circuits :**   **The variables used in this algebra are also called as Boolean variables.**   |  | | --- | | **Digital Circuits - Boolean algebra. Boolean algebra is an algebra, which deals with binary** | | **numbers & binary variables. Hence, it is also called as Binary Algebra or logical Algebra.** |   **x + 0 = x x + 1 = 1 x + x = x x + x’ = 1**  **x.1 = x x.0 = 0**  **x.x = x x.x’ = 0**  **Combinational circuits: Conversion of MUX and Decoders to logic gates:**  **A combination circuit is one that has a "combination" of series and parallel paths for the electricity to flow. Its properties are a combination of the two. In this example, the parallel section of the circuit is like a sub-circuit and actually is part of an over-all series circuit.**   * **In computing and electronic systems, binary-coded decimal (BCD) is a class of binary encodings of decimal numbers where each digit is represented by a fixed number of bits, usually four or eight. Sometimes, special bit patterns are used for a sign or other indications (e.g. error or overflow).** * **Binary Coded Decimal (BCD or “8421” BCD) numbers are made up using just 4 data bits (a nibble or half a byte) similar to the Hexadecimal numbers we saw in the binary tutorial, but unlike hexadecimal numbers that range in full from 0 through to F, BCD numbers only range from 0 to 9, with the binary number patterns of 1010 through to 1111 (A to F) being invalid inputs for this type of display and so are not used as shown below.**   **Design of 7 segment decoder with common anode display:**  **The use of packed BCD allows two BCD digits to be stored within a single byte (8-bits) of data, allowing a single data byte to hold a BCD number in the range of 00 to 99. An example of the 4-bit BCD input ( 0100 ) representing the number “4” is given below** |

|  |  |  |  |
| --- | --- | --- | --- |
| **Date:** | 5/29/20 | **Name:** | **Sathya br** |
| **Course:** | **Python core and advanced** | **USN:** | **4al16ec065** |
| **Topic:** | Input and Output functions | **Semester & Section:** | **6th semester**  **B section** |
| **AFTERNOON SESSION DETAILS** | | | |
| **Image of session** | | | |
| **Report – Report can be typed or hand written for up to two pages.**   * **Introduction** * **print** * **print and string formatting** * **input** * **reading multiple inputs** * **Input and Output functions** | | | |